	Permit #:
	BPS26-000258

	Address:
	1529 S MCKINLEY AVE



1. Obtain all necessary permits for repairs or replacements listed.
EXTERIOR:
· Remove trash and debris away from the property.
· Cut tall grass; trim trees; vegetation away from building.
· Repair damaged kitchen cabinets.
· Weather protection (paint) has deteriorated.
· Repair or replace dry-rot: rafter tails/ facia boards
· Repair or replace broken window(s): permits required for replacement.
· Repair damaged foundation vents.
· Repair damaged walls, ceiling, flooring: crack floor tile (cut hazard)/ hole in wall under kitchen sink
· Repair damaged exterior walls.
· Seal and/or weatherproof exposed wood.
· Repair holes in paved surfaces (unsafe): trip hazards.
· Obtain necessary approvals and permits for:
[ x ] Addition/alteration: Legalize or demolish enclosed patio cover/ Close opening from garage to bedroom
[ ] Remodel
[ ] New structure
[ ] Garage conversion
[ ] As-builts
[ x ] Electrical: Legalize meter panel upgrade
[ x ] Plumbing: Legalize water heater replacement
[ ] Mechanical
[ ] Other
· Provide 36in landing at exterior side door.
ELECTRICAL:
· Main meter service panel and/or sub-panel(s)
· Provide proper bonding of water and gas piping
· Provide 2 ground rods minimum 6ft apart. Permits required.
· Label ALL circuit breakers
· Correct unsafe/hazardous wiring: exposed exterior light fixture wiring.
· Install Ground Fault Circuit Interrupter (GFCI) protection if ANY work has been done with in the past three (3) years, or if GFCI receptacles are not working properly.
[ x ] Kitchen counter-top areas
[ x ] Bathroom sink and vanity area.
[ x ] Garage
[ x ] Exterior
[ x ] Label GFCI receptacle outlets
· Replace or install new light fixture cover(s)
· ANY electrical repairs and/or work MUST be do ne by a California licensed contractor or a qualified electrical journeyman.
WATER HEATER:
· Pressure re lief drain line MUST extend outside of the building or to an APPROVED location.
· Install gas line sediment trap.
· Ensure exhaust vent terminates to the exterior of the building and above roof line.
PLUMBING:
· Flexible p-trap is not permitted for use with kitchen and bathroom sinks. Must use smooth wall piping.
MECHANICAL:
· Heater needs cleaning.
MISCELLANEOUS:
· Repair or replace entry lock(s).
· Submit construction one (1) sets of drawings for unpermitted work.

