212 E Cowan Features
· Large Master Suite on first floor with no bedrooms above, oversized customizable walk-in closet with 10’ island, built-in hampers, full length mirror, 3rd level pull-downs, passage to laundry room. Private entrance to pool.
· 3 En-suite Bedrooms, Game room laundry room & Flex room upstairs.
· 2 large attic areas floored  - lighting for extensive storage.
· Kitchen appliances: Sub-Zero refrigerator/freezer, 48” Wolf Range w/6 burners and 11” griddle, Custom built 60” 6-speed stainless steel 1200 CFM vent hood, Bosch Microwave Drawer, 2 Thermador dishwashers.  
· Summer kitchen & outdoor dining area w/fireplace, 36” DCS grill with rotisserie,1200 CFM vent hood, 24” DCS outdoor refrigerator, custom cabinetry.
· Sliding door system in kitchen opens to pool. Stackable, folding door system in family opens to summer kitchen.
· Large entry pivot door by Western Doors.
· Quartzite counters in kitchen, pantry, butler’s pantry, bar and planning room. Marble counters in master bath and closet island and secondary bathrooms. Quartz countertops in laundry rooms and summer kitchen.
· Family room with Venetian plaster cladded linear fireplace with mood lighting.
· Powder bath with custom concrete sink and Segreto stenciled walls.
· Custom cabinetry throughout.
· 7” wide Cooked Engineered Del Sol French Oak floors with beveled edges installed over Healthy Choice sound and moisture barrier.  
· Natural limestone floors on 1st floor & rear patio, summer kitchen and pool deck.
· 3 car garage with custom showroom finished epoxy finish.
· Commercial Series heavy duty insulated garage doors by Overhead Door Co. with 2 Liftmaster Model 8587 ¾ HP heavy duty operators. 
· 950 lb. capacity elevator.
· 10,867 gallon Heated chlorine pool (3’5” to 5’6” depth) w/water features + heated spa with 10 jets.  Pentair QT blower, skimmers and Whisperflo pool and auxiliary pumps. Pentair Intellitouch control system.
· Landscaping w/engineered drainage, Irrigation system, landscape lighting and robotic lawnmower. Large Live Oak tree in front yard.
· Natural ravine at rear property for separation and privacy.
· Turfed area for low maintenance and year round green area.
· Exterior storage closet on North side of house.
· Whole house over-sized gutters and downspouts tied into drainage. 
· Control 4 Home System w/surround sound in family room, speakers in kitchen, dining, study, outdoor dining, outdoor living, game room, & master. Controller manages all system functions including TV’s, audio system, remote controls, lighting, alarm integration, onscreen navigation & sound equipment.
· In wall Control 4 touch screen in family room. Control 4 door station w/intercom.
· High def exterior IP cameras in 3 locations, expandable for additional cameras.
· Automated Lutron lighting system for most public areas.
· Master Bedroom, Study and Dining Room are pre-wired for automatic drapes.
· Whole house security system by Home Security w/keypad at garage entry.      Pre-wired for keypads at master & entry door. 2 pet immune motion detectors, 11 glass breaks, 8 smoke/heat detectors, 4 combo smoke/CO sensors, outside siren.  
· 2 Tankless Navian water heaters with recirculating pump system.
1” water meter for max flow & pressure with 2” copper service line.
· HVAC: 3 Carrier heat pump 2-stage systems, 3 fan coil units & 3 electric heat strips for emergency heat. Honeywell programmable thermostats.
· Makeup air for 1200 cfm venthood.
· Panasonic exhaust fans in baths and utility.
· Standing seam metal roof. Grace Ice & Watershield over synthetic felt.
· Spray foam insulation encapsulating entire building envelope.
· Windows and doors with lead-coated copper pans and header flashings.
· Interior doors 1-3/4” thickness 3-panel Tru-Stile TS 3000 deluxe styling
· 4 Water Resistant Barriers behind stucco (code requires 2).  Gravity Cavity used to provide drainage plane and totally separate stucco from sheathing.
· Rear accent panel with darkened integral stucco for accent.
· Decorative solid steel panel in front of house.
· Civil Engineered drainage system.
· Foundation pre-treated for termites.
· Foundation engineered w/void boxes, oversized steel reinforcement, void boxes.
· 300 amp overhead electrical service.
· Drywall level 4 finish with USG Tuff Hide primer.






                                     


